Cmp-Mod V01 Created by CvPcb (2012-01-19 BZR 3256)-stable date = 13.1.2013 11:56:41

BeginCmp
TimeStamp = /50F153A0;
Reference = C1;
ValeurCmp = 2nF;
IdModule  = C2;
EndCmp

BeginCmp
TimeStamp = /50F1537C;
Reference = C2;
ValeurCmp = 4.7nF;
IdModule  = C2;
EndCmp

BeginCmp
TimeStamp = /50F15387;
Reference = C3;
ValeurCmp = 0.1muF;
IdModule  = C2;
EndCmp

BeginCmp
TimeStamp = /50F15392;
Reference = C4;
ValeurCmp = 0.1muF;
IdModule  = C2;
EndCmp

BeginCmp
TimeStamp = /50F19548;
Reference = C5;
ValeurCmp = C;
IdModule  = C2;
EndCmp

BeginCmp
TimeStamp = /50F19504;
Reference = C6;
ValeurCmp = CAPAPOL;
IdModule  = C1.5V8V;
EndCmp

BeginCmp
TimeStamp = /50F19513;
Reference = C7;
ValeurCmp = CAPAPOL;
IdModule  = C1.5V8V;
EndCmp

BeginCmp
TimeStamp = /50F1951A;
Reference = C8;
ValeurCmp = CAPAPOL;
IdModule  = C1.5V8V;
EndCmp

BeginCmp
TimeStamp = /50F1951E;
Reference = C9;
ValeurCmp = CAPAPOL;
IdModule  = C1.5V8V;
EndCmp

BeginCmp
TimeStamp = /50F19523;
Reference = C10;
ValeurCmp = C;
IdModule  = C2;
EndCmp

BeginCmp
TimeStamp = /50F1952C;
Reference = C11;
ValeurCmp = C;
IdModule  = C2;
EndCmp

BeginCmp
TimeStamp = /50F19538;
Reference = C12;
ValeurCmp = C;
IdModule  = C2;
EndCmp

BeginCmp
TimeStamp = /50F1953C;
Reference = C13;
ValeurCmp = C;
IdModule  = C2;
EndCmp

BeginCmp
TimeStamp = /50F1AB75;
Reference = C14;
ValeurCmp = C;
IdModule  = C2;
EndCmp

BeginCmp
TimeStamp = /50F1A274;
Reference = D1;
ValeurCmp = LED;
IdModule  = LED-3MM;
EndCmp

BeginCmp
TimeStamp = /50F14559;
Reference = JP1;
ValeurCmp = JUMPER;
IdModule  = PIN_ARRAY_2X1;
EndCmp

BeginCmp
TimeStamp = /50F1468F;
Reference = JP2;
ValeurCmp = JUMPER3;
IdModule  = PIN_ARRAY_3X1;
EndCmp

BeginCmp
TimeStamp = /50F14508;
Reference = K1;
ValeurCmp = CONN_3;
IdModule  = pin_strip_3-90;
EndCmp

BeginCmp
TimeStamp = /50F14639;
Reference = K2;
ValeurCmp = CONN_3;
IdModule  = pin_strip_3;
EndCmp

BeginCmp
TimeStamp = /50F1461B;
Reference = K3;
ValeurCmp = CONN_3;
IdModule  = pin_strip_3-90;
EndCmp

BeginCmp
TimeStamp = /50F14630;
Reference = K4;
ValeurCmp = CONN_3;
IdModule  = pin_strip_3-90;
EndCmp

BeginCmp
TimeStamp = /50F291AB;
Reference = K5;
ValeurCmp = CONN_3;
IdModule  = dc_socket;
EndCmp

BeginCmp
TimeStamp = /50F15631;
Reference = P2;
ValeurCmp = CONN_2;
IdModule  = pin_strip_2-90;
EndCmp

BeginCmp
TimeStamp = /50F14683;
Reference = P3;
ValeurCmp = CONN_2;
IdModule  = mstba_2,5/2-g-5,08;
EndCmp

BeginCmp
TimeStamp = /50F1467C;
Reference = P4;
ValeurCmp = CONN_2;
IdModule  = mstba_2,5/2-g-5,08;
EndCmp

BeginCmp
TimeStamp = /50F14676;
Reference = P5;
ValeurCmp = CONN_2;
IdModule  = mstba_2,5/2-g-5,08;
EndCmp

BeginCmp
TimeStamp = /50F13FEB;
Reference = Q1;
ValeurCmp = STP16NF06;
IdModule  = TO220GDS;
EndCmp

BeginCmp
TimeStamp = /50F13FF7;
Reference = Q2;
ValeurCmp = MOSFET_N;
IdModule  = TO220GDS;
EndCmp

BeginCmp
TimeStamp = /50F14001;
Reference = Q3;
ValeurCmp = MOSFET_N;
IdModule  = TO220GDS;
EndCmp

BeginCmp
TimeStamp = /50F1535B;
Reference = R1;
ValeurCmp = 10k;
IdModule  = SM1206;
EndCmp

BeginCmp
TimeStamp = /50F15344;
Reference = R2;
ValeurCmp = 3k;
IdModule  = SM1206;
EndCmp

BeginCmp
TimeStamp = /50F15352;
Reference = R3;
ValeurCmp = 2k;
IdModule  = SM1206;
EndCmp

BeginCmp
TimeStamp = /50F15361;
Reference = R4;
ValeurCmp = R;
IdModule  = SM1206;
EndCmp

BeginCmp
TimeStamp = /50F152FD;
Reference = R5;
ValeurCmp = 3M;
IdModule  = SM1206;
EndCmp

BeginCmp
TimeStamp = /50F152E7;
Reference = R6;
ValeurCmp = 2k;
IdModule  = SM1206;
EndCmp

BeginCmp
TimeStamp = /50F152F2;
Reference = R7;
ValeurCmp = 2k;
IdModule  = SM1206;
EndCmp

BeginCmp
TimeStamp = /50F154CA;
Reference = R8;
ValeurCmp = 2k;
IdModule  = SM1206;
EndCmp

BeginCmp
TimeStamp = /50F1A286;
Reference = R9;
ValeurCmp = 1k;
IdModule  = R4;
EndCmp

BeginCmp
TimeStamp = /50F1DCDA;
Reference = R10;
ValeurCmp = 0R;
IdModule  = R3;
EndCmp

BeginCmp
TimeStamp = /50F1DCE3;
Reference = R11;
ValeurCmp = 0R;
IdModule  = R3;
EndCmp

BeginCmp
TimeStamp = /50F1DCEF;
Reference = R12;
ValeurCmp = 0R;
IdModule  = R3;
EndCmp

BeginCmp
TimeStamp = /50F15162;
Reference = RV1;
ValeurCmp = POT;
IdModule  = pin_strip_3;
EndCmp

BeginCmp
TimeStamp = /50F13EA9;
Reference = U1;
ValeurCmp = 7805;
IdModule  = LM78XX;
EndCmp

BeginCmp
TimeStamp = /50F13E93;
Reference = U2;
ValeurCmp = ARDUINO_MINI;
IdModule  = arduino_nano_header;
EndCmp

BeginCmp
TimeStamp = /50F142AF;
Reference = U3;
ValeurCmp = LM358;
IdModule  = DIP-8__300;
EndCmp

EndListe
